This was the third experiment.
This time, I opened up all of the flopy drives and "stopped" them which prevented the Amiga OS from seeking and checking for disks being inserted, 
activities that would cause glitches in the audio. Plus, I am now writing to the disk DMA registers directly so I dont want anything to mess that up.

This will only work with the Arduino.

https://rev26.robsmith.dev
https://robsmithdev.co.uk
RobSmithDev

